#include <TimerThree.h>

// This example creates a PWM signal with 25 kHz carrier.
//
// Arduino's analogWrite() gives you PWM output, but no control over the
// carrier frequency.  The default frequency is low, typically 490 or
// 3920 Hz.  Sometimes you may need a faster carrier frequency.
//
// The specification for 4-wire PWM fans recommends a 25 kHz frequency
// and allows 21 to 28 kHz.  The default from analogWrite() might work
// with some fans, but to follow the specification we need 25 kHz.
//
// http://www.formfactors.org/developer/specs/REV1_2_Public.pdf
//
// Connect the PWM pin to the fan's control wire (usually blue).  The
// board's ground must be connected to the fan's ground, and the fan
// needs +12 volt power from the computer or a separate power supply.

const int fanPin = 14;

void setup(void)
{
  Timer3.initialize(40);  // 40 us = 25 kHz
  Serial.begin(9600);
}

void loop(void)
{
  // slowly increase the PWM fan speed
  //
  for (float dutyCycle = 30.0; dutyCycle < 100.0; dutyCycle++) {
    Serial.print("PWM Fan, Duty Cycle = ");
    Serial.println(dutyCycle);
    Timer3.pwm(fanPin, (dutyCycle / 100) * 1023);
    delay(500);
  }
}
