# SdFat: Member List

SdioCard Member List

This is the complete list of members for SdioCard, including all inherited members.

begin(SdioConfig sdioConfig) | SdioCard |
end() | SdioCard | inline
erase(uint32_t firstSector, uint32_t lastSector) | SdioCard | virtual
errorCode() const | SdioCard | virtual
errorData() const | SdioCard | virtual
errorLine() const | SdioCard |
isBusy() | SdioCard | virtual
kHzSdClk() | SdioCard |
readCID(cid_t *cid) | SdioCard | virtual
readCSD(csd_t *csd) | SdioCard | virtual
readData(uint8_t *dst) | SdioCard |
readOCR(uint32_t *ocr) | SdioCard | virtual
readSector(uint32_t sector, uint8_t *dst) | SdioCard | virtual
readSectors(uint32_t sector, uint8_t *dst, size_t ns) | SdioCard | virtual
readStart(uint32_t sector) | SdioCard |
readStart(uint32_t sector, uint32_t count) | SdioCard |
readStop() | SdioCard |
sectorCount() | SdioCard | virtual
status() | SdioCard | virtual
syncDevice() | SdioCard | virtual
type() const | SdioCard | virtual
writeData(const uint8_t *src) | SdioCard | virtual
writeSector(uint32_t sector, const uint8_t *src) | SdioCard | virtual
writeSectors(uint32_t sector, const uint8_t *src, size_t ns) | SdioCard | virtual
writeStart(uint32_t sector) | SdioCard | virtual
writeStart(uint32_t sector, uint32_t count) | SdioCard |
writeStop() | SdioCard | virtual
~BlockDeviceInterface() (defined in BlockDeviceInterface) | BlockDeviceInterface | inlinevirtual